{"text_format":"5","workbook":"xls","n_sheets":5,"sheets":["150W投光灯","洗墙灯1","壁灯","上下打壁灯","防水支架灯"],"props":{"creator":"aa","last_modified_by":"fjzx"},"custom":{"KSOProductBuildVer":"2052-8.1.0.3405"},"not_rendered":{"images":13,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"150W投光灯","index":0,"n_rows":4,"n_cols":6,"rows_kept":4,"merged":[[2,3,3,9]],"flags":["formulas_cached_only"]}
["序号","客户编号","说明","产品型号","产品规格","产品特征"]
[1,"户外","150W投光灯"," NFM013-A11/150W ","345*240","1.铝合金压铸成型灯柱外壳，\n2.灯柱经防腐蚀静电喷涂处理。\n3.高强度硅胶密封圈，适合全体侯使用。  \n4.利于散热。5.广泛适用于各种建筑立面特殊泛光。"]
[2]
[3]

{"sheet":"洗墙灯1","index":1,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[2,3,3,9]],"flags":["formulas_cached_only"]}
["序号","客户编号","说明","产品型号","产品规格","产品特征","安装方式"]
[1,"户外","洗墙灯","NCL005-6W-Y 24V",1000,"1.铝合金压铸成型灯柱外壳，\n2.灯柱经防腐蚀静电喷涂处理。\n3.产品采用3528进口高亮度芯片  \n4.适用于建筑物的轮廓、线条装饰。","明装"]
[2]
[3]

{"sheet":"壁灯","index":2,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[2,3,3,9]],"flags":["formulas_cached_only"]}
["序号","客户编号","说明","产品型号","产品规格","产品特征","安装方式"]
[1,"户外","150W壁灯","NFM038-A/150W 15°","480*270*158","1.内置防眩光圈，\n2.灯柱经防腐蚀静电喷涂处理。\n3.高强度硅胶密封圈，适合全体侯使用。  \n4.带刻度调节转臂。                         ","明装"]
[2]
[3]

{"sheet":"上下打壁灯","index":3,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[2,3,3,9]],"flags":["formulas_cached_only"]}
["序号","客户编号","说明","产品型号","产品规格","产品特征","安装方式"]
[1,"户外","上下打壁灯","NWH013-B1/2x35W/","∮65*280","1.铝合金压铸成型灯柱外壳，\n2.灯柱经防腐蚀静电喷涂处理。\n3.高强度硅胶密封圈，适合全体侯使用。  \n4.灯具结构美观，照明效果极佳。","明装"]
[2]
[3]

{"sheet":"防水支架灯","index":4,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[2,3,3,9]],"flags":["formulas_cached_only"]}
["序号","客户编号","说明","产品型号","产品规格","产品特征","安装方式"]
[1,"户外","T5防水支架","NWF031-A2/21W ",1000,"1.铝合金压铸成型灯柱外壳，\n2.灯柱经防腐蚀静电喷涂处理。\n3.高强度硅胶密封圈，适合全体侯使用。  \n4.维修方便。","明装"]
[2]
[3]